**Section 218.119 Applicability for VOL**

The limitations of Section 218.120 of this Subpart shall apply to all storage containers of volatile organic liquid (VOL) with a maximum true vapor pressure of 0.5 psia or greater in any stationary tank, reservoir, or other container of 151 cubic meters (40,000 gal) capacity or greater, except to vessels as provided below:

a) Vessels with a capacity greater than or equal to 40,000 gallons storing a liquid with a maximum true pressure of less than 0.5 psia;

b) Vessels of coke oven by-product plants;

c) Pressure vessels designed to operate in excess of 29.4 psia and without emissions to the atmosphere;

d) Vessels permanently attached to mobile vehicles such as trucks, rail cars, barges, or ships;

e) Vessels storing petroleum liquids; or

f) Vessels used to store beverage alcohol.

g) Vessels with storage capacity less than 40,000 gallons must comply with Section 218.129(f).

(Source: Added at 18 Ill. Reg. 16950, effective November 15, 1994)