**Section 219.620 Applicability**

a) This Subpart shall apply to all paint and ink manufacturing sources which:

1) Include process emission units not subject to Subparts B, E, F (excluding Section 219.204(l) of this Part), H (excluding Section 219.405 of this Part), Q, R, S, T (excluding Section 219.486 of this Part), V, Y, Z or BB of this Part, and which as a group both:

A) Have maximum theoretical emissions of 91 Mg (100 tons) or more per calendar year of VOM if no air pollution control equipment were used, and

B) Are not limited to less than 91 Mg (100 tons) of VOM emissions per calendar year in the absence of air pollution control equipment, through production or capacity limitations contained in a federally enforceable permit or a SIP revision, or

2) Produce more than 7,570,820 1 (2,000,000 gal) per calendar year of paint or ink formulations, which contain less than 10 percent (by weight) water, and ink formulations not containing as the primary solvents water, Magie oil or glycol.

b) For the purposes of this Subpart, uncontrolled VOM emissions are the emissions of VOM which would result if no air pollution control equipment were used.

(Source: Amended at 17 Ill. Reg. 16918, effective September 27, 1993)