**Section 228.133 Enclosure for Asbestos Construction**

a) The cutting, trimming, fitting or stripping of asbestos-containing material in the construction, alteration or repair of a structure which is done at the site of such structure in an area open to the atmosphere shall be conducted within a special enclosure designed to preclude the escape of asbestos fiber from the immediate area of such enclosure.

b) The mechanical exhaustion of dust from such enclosure to the ambient air is prohibited unless such exhaust system is equipped with a properly sized fabric filter for dust collection or an equivalent device as approved by the Agency.