**Section 244.161 Advisory, Alert and Emergency Levels:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pollutant | Averaging Time | Advisory | Yellow Alert | Red Alert | Emergency |
|  |  |  |  |  |  |
| Sulfur dioxide  (ppm) | 2-hour | 0.30 | -- | -- | -- |
| 4-hour | -- | 0.30 | 0.35 | 0.40 |
|  |  |  |  |  |  |
| (PM10  µg/m3 | 2-hour | 420 | -- | -- | -- |
| 24-hour | -- | 350 | 420 | 500 |
|  |  |  |  |  |  |
| Carbon Monoxide  (ppm) | 2-hour | 30 | -- | -- |  |
| 8-hour | -- | 15. | 30. | 40. |
|  |  |  |  |  |  |
| Ozone (ppm) | 1-hour | 0.12 | 0.20 | 0.30 | 0.50 |
|  |  |  |  |  |  |
| Nitrogen dioxide  (ppm) | 2-hour | 0.40 | -- | -- | -- |
| 1-hour | -- | 0.60 | 1.20 | 1.60 |
| 24-hour | -- | 0.15 | 0.30 | 0.40 |

(Source: Amended at 16 Ill. Reg. 8191, effective May 15, 1992)