**Section 374.205 Influent Pumping**

In the STEP systems, pump well influent piping should enter at the bottom of the well to prevent cascading of septic effluent in order to minimize both odor and corrosion.