**Section 611.125 Fluoridation Requirement**

A CWS adding fluoride to the water must maintain a fluoride ion concentration of 0.7 mg/L as fluorine in its distribution system.

BOARD NOTE: This is an additional State requirement.

(Source: Amended at 47 Ill. Reg. 16486, effective November 2, 2023)