**Section 160.210 Dikes Required – Crude Petroleum**

Tanks or groups of tanks containing crude petroleum or other liquids which have a tendency to boil over shall be diked.