**Section 160.260 Warehouse**

a) Any warehouses erected after April 14, 1977 or converted for the storage of flammable liquids shall have non-combustible walls, roofs and floors and shall be so constructed that refuse cannot accumulate under the floor.

b) Storage of liquids of Class I or II shall not be permitted except in original sealed containers and no transfer of liquids in such containers to other containers shall be made inside the warehouse.

c) Warehouses shall be kept clean, neat and orderly, and free from accumulation of grease and oil spillage.

d) The National Electrical Code as published in NFPA Standard No. 70, (1984) by the National Fire Protection Association, shall govern the electrical installation.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)