**Section 160.300 Electrical Equipment**

a) All electric lights at loading or unloading docks shall be of vapor-proof construction. Electric wiring shall be in sealed conduit at docks and switches shall be of the explosion-proof type or placed at least 20 feet from the docks.

b) All electrical installations, appliances, equipment, and wiring shall conform to the provisions of NFPA # 70 (1984) Chapter 5 and applicable sections thereof.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)