SUBPART M: PROTECTION OF WORKABLE COAL BEDS