**Section 905.30 Approved Private Sewage Disposal Systems**

a) The following systems are approved for private sewage disposal when designed, constructed, operated, and maintained in accordance with this Part:

1) Septic tank, Imhoff tank or aerobic treatment plants followed by:

A) Subsurface seepage field;

B) Seepage bed;

C) Sand filter (buried or re-circulating);

D) Waste stabilization pond;

E) 8 inch or 10 inch gravelless seepage system;

F) Chamber system;

G) Peat filter system; or

H) Subsurface drip irrigation system.

2) Aerobic treatment plant and NSF International/ANSI Standard 40 wastewater treatment systems discharging to supplementary treatment or to the surface, as provided in Sections 905.100 and 905.110.

3) Privies, chemical toilets, re-circulating toilets, incinerator toilets or compost toilets.

4) Holding tanks installed in accordance with Section 905.140.

5) Any other system for which a variance in accordance with Section 905.20(l) has been issued or for which an experimental permit in accordance with Section 905.20(m) has been issued.

6) Illinois raised filter bed preceded by a batch treatment aeration system.

7) Technologies approved by the Department under Section 905.20(t).

b) The Department will maintain a list of alternative components and technologies that have been approved under the Act. This list will be available at http://www.idph.state.il.us/envhealth/prisewage.htm.

c) All other systems or components not listed undert this Part are not approved.

(Source: Amended at 37 Ill. Reg. 14994, effective August 28, 2013)