**Section 930.TABLE A Approved Materials for Water Service Pipe**

|  |  |  |
| --- | --- | --- |
|  | Material | Standard |
|  |  |  |
| 1) | Acrylonitrile Butadiene Styrene (ABS) Pipe | ASTM D 1527-1988 |
|  |  | ASTM D 2282-1988 |
|  | Joints | ASTM D 2235-1988 |
|  | Solvent Cement (1) | ASTM D 2235-1988 |
|  |  |  |
| 2) | Brass Pipe | ASTM B 43-1988 |
|  |  |  |
| 3) | Cast Iron (ductile iron) | ASTM A 377-1984 |
|  | Water Pipe |  |
|  |  |  |
| 4) | Chlorinated Polyvinyl Chloride (CPVC) Pipe | ASTM D 2846-1988 |
|  |  | ASTM F 441-1988 |
|  |  | ASTM F 442-1988 |
|  | Joints | ASTM D 2846-1988 |
|  | Solvent Cement (orange) (1) | ASTM F 493-1988 |
|  |  |  |
| 5) | Copper/Copper Alloy Pipe | ASTM B 42-1988 |
|  |  | ASTM B 302-1988 |
|  |  |  |
| 6) | Copper/Copper Alloy Tubing | ASTM B 88-1988 |
|  |  |  |
| 7) | Polyethylene (PE) Pipe | ASTM D 2239-1988 |
|  |  |  |
| 8) | Polyethylene (PE) Tubing | ASTM D 2737-1988 |
|  |  |  |
| 9) | Polyvinyl Chloride (PVC) Pipe | ASTM D 1785-1988 |
|  |  | ASTM D 224l-1988 |
|  |  | ASTM D 2672-1988 |
|  | Joints | ASTM D 2855-1983 |
|  | Primer | ASTM F 656-1988 |
|  | Solvent Cement (1) | ASTM D 2564-1988 |
|  |  |  |
| (1) | Solvent cement must be handled in accordance with ASTM F 402-1988. |

(Source: Added at 27 Ill. Reg. 15998, effective October 1, 2003)