**Section 350.1005 Requirements for Radiography Equipment Using Radiation Machines**

The control panel of each radiation machine used in industrial radiographic operation shall be equipped with:

a) A locking device to prevent the unauthorized use of the x-ray system or the accidental production of x-rays; and

b) A device that will give a positive indication of the production of x-rays whenever the radiation machine is energized.

(Source: Added at 18 Ill. Reg. 7263, effective May 2, 1994)