**Section 215.103 Abbreviations and Conversion Factors**

a) The following abbreviations are used in this Part:

|  |  |
| --- | --- |
| bbl | barrels (42 gal) |
| C | degrees Celsius or centigrade |
| cu in | cubic inches |
| F | degrees Fahrenheit |
| ft | foot |
| g | gram |
| g/mole | grams per mole |
| gal | gallon |
| hr | hour |
| in | inch |
| K | degrees Kelvin |
| kcal | kilocalorie |
| kg | kilogram |
| kg/hr | kilograms per hour |
| kPa | kilopascals; one thousand newtons per square meter |
| l | liter |
| lb | pound |
| lbs/hr | pounds per hour |
| lbs/gal | pounds per gallon |
| m | meter |
| Mg | megagram, metric ton or tonne |
| min | minute |
| MJ | megajoules |
| mm Hg | millimeters of mercury |
| ml | milliliter |
| ppm | parts per million |
| ppmv | parts per million by volume |
| psi | pounds per square inch |
| psia | pounds per square inch absolute |
| psig | pounds per square inch guage |
| scm | standard cubic meters |
| T | English ton |

b) The following conversion factors have been used in this Part:

|  |  |
| --- | --- |
| English | Metric |

(Source: Amended at 12 Ill. Reg. 815, effective December 24, 1987)