**Section 218.642 Emissions Limitation at Polystyrene Plants**

No person shall cause or allow the emissions of VOM from the material recovery section to exceed 0.12 kg of Volatile Organic Material per 1000 kg of polystyrene resin produced.

(Source: Renumbered from Section 218.877 at 17 Ill. Reg. 16636, effective September 27, 1993)