**Section 725.415 Special Requirements for Containers**

Unless they are very small, such as an ampule, containers must be in either of the following conditions:

a) They must be at least 90 percent full when placed in the landfill; or

b) They must be crushed, shredded, or similarly reduced in volume to the maximum practical extent before burial in the landfill.

(Source: Amended at 29 Ill. Reg. 6389, effective April 22, 2005)