**Section 251.60 Tamper Seals**

The tamper seal must correspond with the color of the certification tag. The tamper seal shall be removed during maintenance and a new tamper seal installed upon completion of maintenance.