**Section 205.1730 Panelboards**

Panelboards serving lighting and appliance circuits shall be located on the same floor as the circuits they serve. This requirement does not apply to any emergency system circuits.

(Source: Amended at 6 Ill. Reg. 6220, effective May 17, 1982)