**Section 760.590 Food Product Thermometers**

Indicating thermometers required for immersion into food or cooking media shall be of metal stem-type construction, numerically scaled, and accurate to ±2°F.