**Section 785.620 Continuous Churn**

All product contact surfaces shall be of noncorrosive material. All nonmetallic product contact surfaces shall comply with 3-A Standards for Plastic, Rubber, and Rubber-Like Materials. All product contact surfaces shall be readily accessible for cleaning and inspection.